## Bode VNA Instrument Driver Readme

To rate this instrument driver, go to the driver download page on the Instrument Driver Network.

#### 1. Overview

Instrument Driver Technology: LabVIEW Plug and Play (project-style)
Manufacturer: OMICRON Lab
Supported Language(s): LabVIEW 2013 or newer
Supported Model(s): Bode 100 & 500
Model(s) Tested: Bode 100 & 500
Interface(s): TCPIP
Software Revision Tested: Bode Analyzer Suite 3.51 SR1
Certified: No
NI Supported: No
Source Code Available: No
Original Release Date: 11/03/2025
Current Revision Date: 16/06/2025

#### 2. Required Software

Some software components need to be installed before using this instrument driver. The minimum versions of these components are listed below, and can be downloaded from the Download Site.
Bode Analyzer Suite 3.51 or newer LabVIEW 2013 or newer
Refer to the LabVIEW Help for more information about software requirements. You access the LabVIEW Help by selecting Help»Search the LabVIEW Help.

#### 3. Known Issues

To report issues or provide feedback about this instrument driver, please send an e-mail to support@omicron-lab.com.
If you have any questions, please contact support@omicron-lab.com for further help.
-------------------------------------------------------------------------------------------------------------------------------

To use this driver:
1. Unzip the folder. It should be named OMICRON Lab Bode VNA Series. Do not rename.
2. Cut or Copy the OMICRON Lab Bode VNA Series folder.
3. Navigate to your LabVIEW folder. It may be found in such a location as: C:\Program Files (x86)\National Instruments\LabVIEW 201x
4. Enter the subfolder \instr.lib
5. Paste the OMICRON Lab Bode VNA Series folder here.
6. That is it! You are ready to begin programming!

-------------------------------------------------------------------------------------------------------------------------------

#### 4. Revision History

The latest version of this and other LabVIEW and LabWindows/CVI instrument drivers can be downloaded at the Instrument Driver Network.
REV 1.0, 01/02/2025
Created by: Oliver Maehr, OMICRON Lab.
Created new driver for Bode 100 & 500 compatible with BAS 3.51 or newer
REV 1.1, 16/06/2025
Modified by: Kurt Andlinger, OMICRON Lab.
Changes:
- USB Driver updated for Bode 100 R2.
New VIs:
- Perform Internal Device Calibration.vi: Allows to perform an internal device calibration (only Bode 100).
- Internal Device Calibration Date.vi: Allows to read the date/time the internal device calibration has been performed (only Bode 100).
REV 1.2, 16/03/2026
Modified by: Kurt Andlinger, OMICRON Lab.
Changes:
- Start Server.vi: It was not always possible to close a SCPI server after starting it via LabVIEW.
- Close Server.vi: It was not always possible to close a SCPI server after starting it via LabVIEW.
- Starting SCPI runner without serial number parameter `-s ` additionally searches beside Bode 100 devices also for Bode 500 USB connected devices.
- Send Trigger.vi: Calculating the visa timeout according to the calculated measurement time.